TP\_CSF\_ValueTypes\_SByte

Reads and writes out an sbyte.

Input

There is a single sbyte *s* on the first line.

Output

There is *s* on the first line.

Examples

|  |  |
| --- | --- |
| Input | Output |
| 0 | 0 |
| -128 | -128 |
| 127 | 127 |